{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["恩平市生活污水处理厂恩平生活污水厂排放口企业监测数据月报202"],"read":"whole","date_system":"1900"}

{"sheet":"恩平市生活污水处理厂恩平生活污水厂排放口企业监测数据月报202","index":0,"n_rows":35,"n_cols":11,"rows_kept":35,"merged":[[0,0,0,10],[1,0,2,0],[1,1,1,2],[1,3,1,4],[1,5,1,6],[1,7,1,8]]}
["恩平市生活污水处理厂恩平生活污水厂排放口企业监测数据月报20212"]
["监测时间","COD",null,"氨氮",null,"总磷",null,"总氮",null,"pH","水流量"]
[null,"浓度(mg/L)","排放量(千克)","浓度(mg/L)","排放量(千克)","浓度(mg/L)","排放量(千克)","浓度(mg/L)","排放量(千克)","","吨"]
["2021-02-01 00:00:00","15.325","368.269","1.372","32.027","0.14","3.354","3.865","91.913","6.614","24030.936"]
["2021-02-02 00:00:00","14.836","352.852","1.428","32.219","0.126","2.964","4.874","114.73","6.606","23838.342"]
["2021-02-03 00:00:00","13.716","322.106","1.706","39.121","0.116","2.734","4.865","115.305","6.591","23696.911"]
["2021-02-04 00:00:00","13.717","330.775","0.823","18.733","0.105","2.523","5.205","125.819","6.589","24153.96"]
["2021-02-05 00:00:00","13.934","330.165","1.04","23.267","0.101","2.38","4.998","118.762","6.58","23714.124"]
["2021-02-06 00:00:00","14.062","336.801","1.306","30.371","0.103","2.468","4.319","102.946","6.614","23927.511"]
["2021-02-07 00:00:00","14.382","336.839","1.164","26.812","0.105","2.465","4.006","93.902","6.643","23449.791"]
["2021-02-08 00:00:00","13.573","321.565","0.869","20.461","0.088","2.083","4.556","108.154","6.631","23716.971"]
["2021-02-09 00:00:00","13.374","321.853","0.8","19.264","0.077","1.849","5.561","133.795","6.61","24074.595"]
["2021-02-10 00:00:00","12.322","294.12","1.954","44.768","0.099","2.318","6.094","145.036","6.728","24019.953"]
["2021-02-11 00:00:00","8.619","210.167","0.221","5.385","0.068","1.666","4.715","115.321","6.776","24370.851"]
["2021-02-12 00:00:00","7.936","193.801","0.195","4.759","0.077","1.892","3.761","91.475","6.712","24392.439"]
["2021-02-13 00:00:00","9.657","230.952","0.871","20.77","0.088","2.094","4.739","113.371","6.567","23863.479"]
["2021-02-14 00:00:00","10.381","249.098","0.876","20.511","0.098","2.354","5.233","125.77","6.597","24031.026"]
["2021-02-15 00:00:00","11.488","279.018","0.951","22.666","0.104","2.514","5.62","135.945","6.531","24213.447"]
["2021-02-16 00:00:00","11.213","268.042","0.859","20.452","0.1","2.37","5.94","141.789","6.484","23871.822"]
["2021-02-17 00:00:00","10.321","247.901","2.016","48.432","0.092","2.212","6.462","155.499","6.569","24053.387"]
["2021-02-18 00:00:00","10.549","254.641","0.96","23.082","0.075","1.811","6.231","150.217","6.536","24115.554"]
["2021-02-19 00:00:00","10.788","259.851","0.486","11.88","0.073","1.755","7.654","183.87","6.455","24056.724"]
["2021-02-20 00:00:00","9.664","231.729","0.221","5.405","0.073","1.753","7.552","181.255","6.521","24035.703"]
["2021-02-21 00:00:00","8.541","208.615","0.371","9.027","0.068","1.662","7.728","188.764","6.458","24432.888"]
["2021-02-22 00:00:00","13.126","320.685","0.28","6.914","0.071","1.735","6.882","166.822","6.481","24232.161"]
["2021-02-23 00:00:00","20.091","481.715","0.119","2.837","0.086","2.066","5.351","128.661","6.599","23983.935"]
["2021-02-24 00:00:00","20.355","490.334","0.146","3.551","0.089","2.136","3.53","85.156","6.699","24079.11"]
["2021-02-25 00:00:00","20.73","502.94","0.284","6.836","0.091","2.2","3.561","86.472","6.588","24262.14"]
["2021-02-26 00:00:00","22.322","534.917","0.368","8.741","0.112","2.674","4.178","100.164","6.584","23957.13"]
["2021-02-27 00:00:00","20.327","472.088","0.709","16.626","0.132","3.057","3.279","76.313","6.641","23233.845"]
["2021-02-28 00:00:00","20.737","491.085","0.176","4.209","0.121","2.859","2.601","61.221","6.771","23646.03"]
["平均值","13.789","330.104","0.806","18.897","0.096","2.284","5.120","122.802","6.599","23980.527"]
["最大值","22.322","534.917","2.016","48.432","0.140","3.354","7.728","188.764","6.776","24432.888"]
["最小值","7.936","193.801","0.119","2.837","0.068","1.662","2.601","61.221","6.455","23233.845"]
["排放总量","","9242.924","","529.126","","63.948","","3438.447","","671454.765"]